STAR MICRONICS GEMINI-10X - CWC printer definition file

Note: DIP switches 2-2, 2-3, and 2-4 must all be set "OFF"

      For the SG-10/15, these switches must all be set "ON"


Print settings
=============================================================================
MaxPrintCols=/80                       number of characters per line

PuzzlePrint=/027/035                   use full 8 bits for character data
PuzzlePrint=/027/053                   select "standard" ROM character set

EndPrint=/012                          form feed

SpacingTHalfBox=/027/065/003           select  3/72 in. spacing
SpacingBHalfBox=/027/065/003           select  3/72 in. spacing
SpacingWholeBox=/027/065/006           select  6/72 in. spacing
SpacingClues=/027/065/012              select 12/72 in. spacing
SpacingNormal=/027/065/012             select 12/72 in. spacing

SpecialNumbersON=/027/083/000          set superscript ON
SpecialNumbersOFF=/027/084             set superscript OFF

SpecialLettersON=/027/083/000          set superscript ON
SpecialLettersOFF=/027/084             set superscript OFF


Character set
=============================================================================
BoxTLCor=/240                          this character set is unique to the
BoxTRCor=/242                          GEMINI-10; it is used here because
BoxBLCor=/246                          this printer does not support the
BoxBRCor=/247                          IBM character set
BoxTopBot=/241
BoxSide=/245
BoxLTee=/244
BoxRTee=/249
BoxTTee=/243
BoxBTee=/248
BoxCross=/250
BoxLFill=/234
BoxCFill=/239
BoxRFill=/233
BoxSpace=/032
