generic EPSON printer (standard ASCII char set) - CWC printer definition file


Print settings
=============================================================================
MaxPrintCols=/80                       number of characters per line

EndPrint=/012                          form feed

SpacingTHalfBox=/027/065/004           select  4/72 in. spacing
SpacingBHalfBox=/027/065/004           select  4/72 in. spacing
SpacingWholeBox=/027/065/008           select  8/72 in. spacing
SpacingClues=/027/065/012              select 12/72 in. spacing
SpacingNormal=/027/065/012             select 12/72 in. spacing

SpecialNumbersON  =/027/083/000          set superscript ON
SpecialNumbersOFF  =/027/084             set superscript OFF


Character set
=============================================================================
BoxTLCor=/043                          since only the standard ASCII
BoxTRCor=/043                          characters are supported, the
BoxBLCor=/043                          boxes are drawn with only three
BoxBRCor=/043                          simple characters: "+", "-", and "|"
BoxTopBot=/045
BoxSide=/124                           note that the LEFT and RIGHT BOX
BoxLTee=/043                           FILL characters are defined as a
BoxRTee=/043                           SPACE, since nothing else is thin
BoxTTee=/043                           enough to print next to the "|"
BoxBTee=/043                           without obscuring it
BoxCross=/043
BoxLFill=/032
BoxRFill=/032
BoxCFill=/042
BoxSpace=/032
