TOSHIBA P1351 - CWC printer definition file


Print settings
=============================================================================
PuzzlePrint=/027/061                   coded graphics ON

CluePrint=/027/063                     coded graphics OFF

EndPrint=/027/063                      coded graphics OFF
EndPrint=/012                          form feed

SpacingTHalfBox=/027/076/048/051       select  3/48 in. spacing
SpacingBHalfBox=/027/076/048/050       select  2/48 in. spacing
SpacingWholeBox=/027/076/048/053       select  5/48 in. spacing
SpacingClues=/027/076/048/056          select  8/48 in. spacing
SpacingNormal=/027/076/048/056         select  8/48 in. spacing

SpecialTitleON=/027/063                coded graphics OFF
SpecialTitleOFF=/027/061               coded graphics ON

SpecialNumbersON=/027/063              coded graphics OFF
SpecialNumbersOFF=/027/061             coded graphics ON

SpecialLettersON=/027/063              coded graphics OFF
SpecialLettersOFF=/027/061             coded graphics ON


Character set
=============================================================================
BoxTLCor=/240                          this character set is unique to the
BoxTRCor=/242                          P1351; it is used here because this
BoxBLCor=/246                          printer does not support the IBM
BoxBRCor=/247                          character set
BoxTopBot=/241
BoxSide=/245
BoxLTee=/244
BoxRTee=/249
BoxTTee=/243
BoxBTee=/248
BoxCross=/250
BoxLFill=/234
BoxCFill=/239
BoxRFill=/233
BoxSpace=/224
